**Printers at SPOL**

We currently have two printers for access on the network at SPOL. Both are setup to be a standard TCP/IP Printer. Depending on your operating system you may have the drivers already preinstalled. Most version of the Mac OS have it preinstalled as well as Centos and Windows 7. With many older operating systems you may need to download drivers from HPs website here - <http://www8.hp.com/us/en/support-drivers.html>.

Color Printer:

Type – HP Laserjet 2605n

IP Address – 192.168.4.36

Hostname – Color.gate.rtf

Location – The location of the printer is in the SCC above the ENG computer.

B/W Printer:

Type – HP Laserjet 4050n

IP Address – 192.168.4.37

Hostname – Mono.gate.rtf

Location – The location of the printer is in the Annex.